When the ring is horizontal the disk can be rotated to adjust the power level.

When horizontal, the disk and ring form an annular opening which area is ¼ the area of the fuel reactor chamber.

When the disk and ring are vertical the stove is at full power.