Rods may be different cross sectional shapes, but they need to be straight.

Top of stove

Make the rods long enough to leave room to get the fuel into the stove.

Metal rods bent and welded would leave more room to work and might be easier to use.